Level 0 Modules

|  |  |
| --- | --- |
| *Module* | E-Wand |
| *Inputs* | - User Control: on/off  - Image(any format, size, etc) |
| *Outputs* | Complete display including rotation and flashing LEDs |
| *Functionality* | Receives an image and displays it in a cylindrical format that can be used for advertisement and as a signal for help. |

The E-Wand will first accept an input of an image. After accepting the user input the E-Wand will recognize that it has an input and translate that into a cylindrical display that accurately reflects the desired image.